Skip to content

# JEISYS TRI-BEAM K Q-Switched Nd

JEISYS TRI-BEAM K Q-Switched Nd:YAG Laser
Tri-Beam Q-SWITCH LASER
The Most Advanced and Advantageous Features of Q-Switched Nd:
YAG Laser
Rich-PTP Technology
Gen Technique by using Quasi-Long Pulse
Laser Parameter
Laser Medium Nd:
YAG (Q-switched)
Operating Parameters Q-Switched and Quasi-Long Pulse
Wave Length 1064/532 nm
Energy at end Of Hanpiece
Q-switched PTP Mode 1064nm 1,6Joule
Top Hat mode 1064nm 1,2Joule
532nm 450Joule
Gaussian mode 1064nm 1,5Joule
Quasi-Long Pulse 1064nm 3,5Joule
Pulse Width
Q-Switched 5-10 ns
Quasi-Long Pulse 300µs
Repetition Rate Single shot, 1-20Hz (pulse per second)
Beam Profile True Flat-Top
Energy Calibration Internal
Spot Sizes(auto sensing) Zoom Handpiece 1064nm 2mm-10mm
532 nm 2mm-10mm
Collimate Handpiece 7mm
Fractional Handpiece 5mmx 5mm(81spots)
Physical Parameters
Electrical Power 220 V, Single Phase, 50/60Hz, 20 Amps at 20V AC
Weight 110kg
Dimensions 954mm(H) x 440mm(W) x 950mm(L) without articulated arm
Beam Delivery Articulated arm with up to 240cm reach, 7-joint, 3600 rotation
Cooling Closed cycle water to air heat exchange

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info