Skip to content

# Siemens Acuson S3000 18L6 HD

Siemens Acuson S3000 18L6 HD Transducer
The Siemens 18L6 HD Linear Array transducer has a frequency range of 6.0 MHz. – 18.0 MHz. and supports the following applications: Breast, Musculoskeletal, Urology, Vascular,
The Siemens 18L6 HD transducer is compatible with: Siemens Acuson S3000 ultrasound systems.
Form Factor: Linear Array
Applications: Breast, Musculoskeletal, Urology, Vascular
Frequency Range: 6.0 – 18.0 MHz.
Compatibility: Siemens Acuson S3000

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info