Skip to content

# Siemens Acuson P8-4

Siemens Acuson P8-4 Transducer
MFG in 2019
8-4 MHz Phased Array Transducer for Abdomen, Neonatal Echo, Neonatal Head, Pediatric Abdomen, Pediatric Echo, Renal

### Transducer Details:

Frequency Bandwidth: 2.7 – 8.0 MHz
Selectable 2D Frequencies: 3.8, 5.3, 6.7 MHz
Selectable THI Frequencies: 2.7, 3.1 MHz
Selectable Color Doppler Frequencies: 3.6, 4.4 MHz
Selectable PW Doppler Frequencies: 3.6, 4.4 MHz
Steerable CW Doppler Frequencies: 3.6 MHz
Number of Elements: 64
Footprint: 9.6 mm
Maximum Field of View: 90º
Maximum Display Depth: 140 mm
Biopsy Guide: Not available

### Design Attributes:

Wide bandwidth curved array transducer
User-selectable MultiHertz imaging
Ergonomically designed form factor
Lightweight transducer with flexible cable

### Applications:

Abdomen , Neonatal Echo
Neonatal Head ,Pediatric Abdomen
Pediatric Echo, Renal

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info