Skip to content

# APOGEE 5500

APOGEE 5500 HAIR REMOVAL LASER AVAILABLE IN KOREA WITH EXCELLENT CONDITION
Flashlamp changed with new lamp .
Cynosure Apogee 5500 Alexandrite Laser 755 nm
The Cynosure Apogee 5500 permanently removes hair on a wide variety of skin types using a 755 nm Alexandrite Laser. Additionally, it can treat benign epidermal pigmented lesions such as age spots, sunspots and freckles. Effective, Safe And Gentle.
Cynosure Apogee 5500 Specifications
Laser Type: Flashlamp, Excited Solid State Alexandrite Laser
Wavelength: 755 nm
Optical Output: Fused Silica Optical Fiber
Output Mode: Multi-mode
Cooling Method: Circulated WATER with heat exchange
Pulse Width: 0.5 to 300 msec
Maximum Fluence / Energy
15 mm – 25 J/cm2
12 mm – 35 J/cm2
10 mm – 50 J/cm2
5 mm – 100 J/cm2
Repetition Rate: 1 to 3 Hz
Aiming Beam
Source: LED
Wavelength: 505 nm (blue-green)
Maximum Delivered Output Power: less than 5.0 mW
Electrical Info: 200 – 220 VAC | 50 – 60 Hz | 30 A | Single Phase
Dimensions: 15″ W x 25 1/4″ D x 41″ H
Weight: 180 lbs
Cynosure Apogee 5500
Handpieces with Spot Sizes 5 mm, 12 mm and 15 mm
Footswitch, Key
Operator Manual
(2) Operator Eyewear

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info