Skip to content

# L-BEAM HAIR REMOVAL

REFURBISHED LONG PULSE ND:YAG HAIR REMOVAL LASER L-BEAM
HAIR REMOVAL 1064nm Wavelength L-BEAM
LASER

### Key Features:-

1064nm Wavelength Long pulse ND:YAG Permanent Hair removal on all Skin Type Skin Tighting&Fine Wrinkle reduction Vascular Lesions Facial Veins

### SPECIFICATION:-

Irradiation Type Optic Fiber Long pulse
Wavelength 1064
Pulse Duration Max15ms (3 Pulses)
Frequency Max10Hz (Genesis Mode)
Cooling system Gas cooling
Spot Size 2mm~15mm
Maximum Energy 100J

1. L-BEAM LASER have very easy 4 Programs use with touch screen Method
2. VASCULAR REMOVAL MODE
3. HAIR REMOVAL MODE
4. SKIN REJUVENATION MODE
5. GENESIS MODE for Face lifting,Acne Redness , Flushing,Skin Texture, Skin Tone.

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info