Skip to content

# GE 6TC-RS TEE PROBE

GE 6TC-RS TEE PROBE AVAILABLE FOR SALE
6Tc-RS TEE probe
The GE 6Tc-RS is a transesophageal echocardiography (TEE) probe that is compatible with the GE Vivid i system and designed to be used for adult cardiac applications.
Bandwidth: 2.9 – 8 MHz
Applications: Cardiac
Imaging Modes: 2D, Harmonics, M-Mode, Color Doppler, PW Doppler, CW Doppler, Contrast Imaging, TVI, Tissue Tracking, TSI
Footprint: L45 x W14 (x H12.5) mm (Logiq e), 12 x 14 mm, length 45 mm (Vivid i, q)
Field of View: 90°
Compatibility: Logiq e, Vivid E9, Vivid i, Vivid i n, Vivid q

# Contact Us

### Addresses

318 Diart Gallery A Dong , Sohyang Ro 119 , Wonmi-gu, City : Bucheon-si Province : Gyeonggi-do , South Korea

### Phone Number

+82-10-2320-8582

### Email

sonomedex@gmail.com

### Timing

Monday to Friday: 10am to 7pm
Saturday: 10am to 4pm Sunday: 12am to 4pm

## Booking Form

First Name
Last Name
Email
Phone
Additional Info